**Eco-Friendly Zr-Metal Organic Framework Materialfor Efficient**

**Remediation of Different Types of Dyes**

Hassan Shokry Hassan 1,2\*and Marwa F. Elkady3,4, Kamal E. Diab5,Saad Mahmoud5, Raya Al-Dadah5

*\*1Environmental Engineering Department, Egypt-Japan University of Science and Technology, New Borg El-Arab City, Alexandria 21934, Egypt.Telephone number:01282305425,E-mail:* [*hassan.shokry@ejust.edu.eg*](mailto:hassan.shokry@ejust.edu.eg)

*2Electronic Materials Research Department, Advanced Technology and New Materials Research Institute (ATNMRI), City of Scientific Research and Technological Applications (SRTA-City), New Borg El-Arab City, Alexandria 21934, Egypt.*

*3Chemical and Petrochemical Engineering Department, Egypt-Japan University of Science and Technology (E-JUST), New Borg El-Arab City, Alexandria 21934, Egypt.*

*4Fabrication Technology Research Department, Advanced Technology and New Materials Research Institute (ATNMRI), City of Scientific Research and Technological Applications (SRTA-City), New Borg El-Arab City, Alexandria 21934, Egypt.*

*5Department of Mechanical Engineering, University of Birmingham, Edgbaston, Birmingham B152TT, UK*

**Abstract**

Bio-MOF using aspartic acid as an organic linker and water as a solventwas performed to create an eco-friendly material. The chemical composition, structure,and morphology of the synthesized zirconium Bio-MOF (MIP-202) was evaluated using X-raydiffraction (XRD), energy dispersive X-ray (EDX) spectroscopy, transmission electron microscopy(TEM), scanning electron microscopy (SEM), and X-ray photoelectron spectroscopy (XPS).The adsorption capability of the synthesized Zn-adeninate bio-MOF was confirmed by itsnotable surface area of 52.62m2 g−1 and total pore volume of 0.183 cm3 g−1. The bio-MOF adsorption profiles of anionic directred 81 (DR-81) and cationic methylene blue (MB) dyes were investigated under different operating parameters. The optimumdosages of Zn-adeninate bio-MOF were 0.5 g L−1 and 1 g L−1 for MB and DR-81 decolorization, respectively.Kinetic parameters were well-fitted with pseudosecond-order kinetics, and the adsorption process was described by the Freundlich isotherm.

*Keywords: zirconium Bio-MOF;adsorption process;ecofriendly materials; Kinetic models; methylene blue*

**Acknowledgments**

This work was supported by The British Council under Research Environment Links call for project entitled "Capacity Building in Egypt for Enhancing water availability, food security and renewable energy using MOF adsorption heat pumps” (Grants no. 871105921).